CertificateNo. :\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Date 03.07.2020

**CERTIFICATE OF WEIGHT**

At the request of Indo International Trading FZCO, Jebel Ali, Dubai, UAE, we, through our associates in Malaysia have attended the weighment and loading survey of **Graphite Electrodes** and certify as under:

SHIPPERS : SHOWA DENKO CARBON GERMANY GMBH

WERNER-VON-SIEMENS-STRASSE 18

86405 MEITINGEN, GERMANY.

CONSIGNEE : TO THE ORDER OF AHLI BANK SAOG, OMAN

BUYERS : JINDAL SHADEED IRON & STEEL LLC

SOHAR PORT, PLOT NO.12, P.O.BOX 404,

P.C.322, FALAJ AL QABAIL, SOHAR,

SULTANATE OF OMAN

TEL : 00968 26850403

FAX: 00968 26850438

DESCRIPTION OF THE GOODS : GRAPHITE ELECTORDE 750 x 2700 MM WITH

NIPPLES 406 x 610 MM, T4

20 CRATES . 4 X 40FT CONTAINERS

SEAWORTHY STANDARD EXPORT PACKING WITH

EACH CRATE CONTAINS TWO (2) ELECTRODES .

MATERIAL CODE : 10000574

PO Number : 4500019526 DATED 29.03.2020

VESSEL NAME : MV BLANDINE 893E

LOADING PORT : PORT KLANG, MALAYSIA

DISCHARGE PORT : PORT SOHAR, SULTANATE OF OMAN

B/L NUMBER : EGLV091030257160 DATED JUN 30, 2020

DATE OF INSPECTION : 28th JUNE 2020.

At the time of our inspection, the sellers presented for our inspection the following Electrodes with Nipples for our inspection. The materials were then inspected for :

* Measuring and weighing
* Witnessing the installation of the nipple
* Witnessing of the crating progress
* Visual Condition
* Packing and Marking

 Contd…2

CertificateNo. :\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Page : 2

|  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **CRATE**  **NO** | **NO.OF PIECES** | **MONOTRODE**  **ID** | **ELECT-ROD**  **+**  **NIPPLE**  **WEIGHT**  **(MT)** | **TOTAL**  **NET WEIGHT**  **(MT)** | **TARE**  **WEIGHT**  **(KGS)** | **GROSS**  **WEIGHT (MT)** | **LENGTH**  **(MM)** | **WIDTH**  **(MM)** | **HEIGHT**  **(MM)** |
| 1 | 2 | 1115054690  1115043390 | 2.309  2.276 | 4.585 | 104 | 4.689 | 3340 | 1590 | 880 |
| 2 | 2 | 1115045290  1115054190 | 2.283  2.310 | 4.593 | 104 | 4.697 | 3340 | 1590 | 880 |
| 3 | 2 | 1115054390  1115054190 | 2.288  2.308 | 4.596 | 104 | 4.700 | 3340 | 1590 | 880 |
| 4 | 2 | 1115058390  1115054490 | 2.305  2.311 | 4.616 | 104 | 4.720 | 3340 | 1590 | 880 |
| 5 | 2 | 1115053290  1115056790 | 2.293  2.278 | 4.571 | 104 | 4.675 | 3340 | 1590 | 880 |
| 6 | 2 | 1115055490  1115052990 | 2.294  2.306 | 4.600 | 104 | 4.704 | 3340 | 1590 | 880 |
| 7 | 2 | 1115056690  1115057590 | 2.290  2.299 | 4.589 | 104 | 4.693 | 3340 | 1590 | 880 |
| 8 | 2 | 1115057490  1115057190 | 2.281  2.240 | 4.521 | 104 | 4.625 | 3340 | 1590 | 880 |
| 9 | 2 | 1115053090  1115054790 | 2.312  2.296 | 4.608 | 104 | 4.712 | 3340 | 1590 | 880 |
| 10 | 2 | 1115044190  1115044290 | 2.305  2.298 | 4.603 | 104 | 4.707 | 3340 | 1590 | 880 |
| 11 | 2 | 1115045490  1115045390 | 2.290  2.301 | 4.591 | 104 | 4.695 | 3340 | 1590 | 880 |
| 12 | 2 | 1115044590  115043990 | 2.304  2.278 | 4.582 | 104 | 4.686 | 3340 | 1590 | 880 |
| 13 | 2 | 1115044390  1115044690 | 2.303  2.295 | 4.598 | 104 | 4.702 | 3340 | 1590 | 880 |
| 14 | 2 | 1115054890  1115044490 | 2.304  2.259 | 4.563 | 104 | 4.667 | 3340 | 1590 | 880 |
| 15 | 2 | 1115053490  1115066690 | 2.311  2.240 | 4.551 | 104 | 4.655 | 3340 | 1590 | 880 |
| 16 | 2 | 1115044890  1115053690 | 2.258  2.318 | 4.576 | 104 | 4.680 | 3340 | 1590 | 880 |
| 17 | 2 | 1115058290  1115055090 | 2.308  2.303 | 4.611 | 104 | 4.715 | 3340 | 1590 | 880 |
| 18 | 2 | 1115043290  1115056890 | 2.317  2.300 | 4.617 | 104 | 4.721 | 3340 | 1590 | 880 |
| 19 | 2 | 1115055190  1115051790 | 2.301  2.315 | 4.616 | 104 | 4.720 | 3340 | 1590 | 880 |
| 20 | 2 | 1115054990  1115052790 | 2.290  2.303 | 4.593 | 104 | 4.697 | 3340 | 1590 | 880 |
|  |  |  |  | 91.780 | 2080 | 93.860 |  |  |  |

Contd..3

CertificateNo. :\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Page : 3

The above 20 crates were stuffed into 4 x 40 FT Containers as per detailed here-below:-

|  |  |  |  |
| --- | --- | --- | --- |
| CONTAINER NO | NO OF CRATES | GROSS WEIGHT IN KGS | SEAL NO |
| BSIU9507225 | 05 | 23405.000 | EMCGWB1409 |
| EITU1894192 | 05 | 23533.000 | EMCGWC0959 |
| TCNU3022138 | 05 | 23441.000 | EMCGWC0369 |
| TCLU4925244 | 05 | 23481.000 | EMCGWC1299 |
|  | 20 | 93860.000 |  |

Photographs taken during the stuffing are as following :-

|  |  |
| --- | --- |
|  |  |
| View of Graphite Electrodes in Crates | Marking on Wooden Crates |
|  |  |
| Fumigated Stamp On Wooden Crate. | Bottom Base with Connected Stud Bolts. |

Contd..4

CertificateNo. :\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Page : 4

Date : 03.07.2020

|  |  |
| --- | --- |
|  |  |
| Crates Stacked Onto Wooden Bottom Base | Metal strapping used to secure and tight around the crates on wooden bottom base |
|  |  |
| Crates stacked onto wooden bottom base and Meta strapped | 3T forklift utilized to push and load the crate into the container. |
|  |  |
| View of lashing affixed | Unifixx W450-5000 daN /11000lbs lashing belt being used to secure the Crates |

Contd..5

CertificateNo. :\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Page : 5

|  |  |
| --- | --- |
|  |  |
| View of choking applied | View of chocking applied to the Crates upon completion of loading |
|  |  |
| View of empty container No. TCLU4925244 | View of Prefix |
|  |  |
| Container No. TCLU4925244 upon completion of stuffing and lashing. | Container No. TCLU4925244 with one door closed upon completion of loading and lashing |

Contd..6

CertificateNo. :\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Page : 6

|  |  |
| --- | --- |
|  |  |
| Container Door closed and sealed | View of Seal No.EMCGWC1299 affixed |
|  |  |
| Vew of empty container No. TCNU3022138 | View of Prefix |
|  |  |
| Container No. TCNU3022138 after loading and lashing | Container No.TCNU3022138 with one door closed upon completion of loading and lashing |

Contd..6

Certificate No. :\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Page : 6

|  |  |
| --- | --- |
|  |  |
| Container No.TCNU3022138 closed and sealed | View of Seal No.EMCGWC0369 |
|  |  |
| View of empty container No.BSIU9507225 | View of prefix |
|  |  |
| Container No.BSIU-9507225 upon completion of stuffing and lashing | View of one door closed after loading and lashing |

Contd..7

CertificateNo. :\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Page : 7

|  |  |
| --- | --- |
|  |  |
| Container No.BSIU9507225 closed and sealed | View of Seal No.EMCGWB1409 affixed |
|  |  |
| View of empty container No. EITU1894192 | View of prefix |
|  |  |
| Container No. EITU1894192 upon completion of loading and lashing | Container No. EITU1894192 with one door closed after loading and lashing |

Contd..8

CertificateNo. :\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Page : 8

|  |  |
| --- | --- |
|  |  |
| Container No.EITU1894192 both door closed and sealed. | View of Seal No.EMCGWC0959 |
|  |  |

The above inspected Electrodes were then packed in our presence in standard customised sea worthy crated packing materials for Containerized transportation to the destination. The same were found to be in order.

**Based on our findings, the subject material as above confirmed to the Packing list provided for this shipment. This report reflects our findings at the time, date and place of inspection.**

**For AgriMin Control International Pte. Ltd**