Dear Barathi

Many thanks for the nomination and support, we confirm attendance

We understand that job will commence tomorrow. As discussed in previous 840 bags nomination, no sampling was performed for analysis purpose, random samples were taken just to monitor discoloured cargo and it was not retained.

In this nomination I understand you require us to take samples during stuffing ? and need to send for analysis. Please confirm as we need to expedite sampling and testing accordingly.

Also whether the sampling to be performed for entire consignment as one analysis representing 32 FCL certificates ?

Regards

Manoj

**From:** Barathi <barathi@valencyinternational.com>   
**Sent:** Friday, 4 September 2020 1:28 PM  
**To:** Manoj Kewalramani <manoj.kewalramani@agrimincontrol.com>  
**Cc:** 'Vishnu, VITPL' <vishnu@valencyinternational.com>; AGRIMIN INDO <operations-indo@agrimincontrol.com>; Siddharth Amin <siddharth.amin@agrimincontrol.com>; 'Priyanka' <priyanka@valencyinternational.com>; 'Barathi' <barathi@valencyinternational.com>  
**Subject:** Bagging - Stuffing Inspection nomination - Portklang (New Nomination)

Dear Mr. Manoj,

Product: Granular urea

Contact Details: Mr. Nazari

Location:

Berjaya Baja Servis Sdn Bhd

Located at PT4231 (Lot 26725),

Lingkaran Sultan Hishamuddin,

Kawasan Perusahaan Selat Klang Utara,

42000 Pelabuhan Klang (nearby Hainan Village),

Selangor Darul Ehsan, Malaysia.

Booking Number: MCLPKGRGN2000263

POL: Port Klang, Malaysia

POD: Yangon, Myanmar

Marking & Quantity:

Blue Phyo Bag – 29 to 32  FCL

**Basic requirement for POL Inspection as follows:**

**Container:**

Checking the cleanliness of containers & its sound condition before stuffing.

Share with us the stages of picture starting from empty containers till the container sealed.

Rejection of containers that are damaged and not seaworthy.

Verification of quantity against weigh bridge slips .

Actual counting of Bags before sealing the containers.

Rejection of cargo if it deviates from the specification.

Reading of Container wise Gross Weight & Net weight.

Inspection seal is mandatory and picture to be taken to show container number & Inspection seal number & Shipping line seal number.

**Bagging:**

Ensure no visible dirt, severely discoloured urea and lumps are removed.

Ensure cargo packed in bags is free flowing & cargo is as pure as possible but to maintain same packing rate as trial

Check weighing machine calibration before allowing for bagging.Net weight should be **50kgs (no minus tolerance)**

Verification of Bag marking and Bag Drop tests to ensure they are sound.

Rejection of Torn or Partial stitching bags. Bags should be double stitched.

1% of empty extra bags are required. Once stuffing complete, pls advise container number where  empty extra bags kept along with total number of empty extra bags in each container

Foreign particles limited to 1% max.

**Quality:**

The below analysis to be performed on the one composite sample taken during stuffing.

**Specifications:**

 Analysis on one composite sample drawn and the details as following:

Granular UREA

Moisture                                                       :             1.0% maximum

Nitrogen                                                       :             46% minimum

Biuret                                                             :             1.0% maximum

Physical condition                                       :             Granular, free flowing non-caking, White in colour.

...............................................................................................................................................................................................................................................................................................

**Note :**

* Pls stop bagging or loading of cargo immediately and contact us in the event that there is deviation from any of the above requirements.
* Inspection status to be update to us on daily basis and testing report to receive prior to the container loading into the vessel.
* Issuance of final certificates: Certificate of Quality, Quantity and Analysis in 1 original and 2 copies.

Warm Regards,

Barathi

|  |  |
| --- | --- |
|  | **Barathi**  Valency International Pte Ltd,  10 Anson Road, 18-26, International Plaza, Singapore 079903  Direct +65 6692 9487  Mobile +65 9750 8506  Board +65 6692 9460   Fx +65 6223 4252  Email: [barathi@valencyinternational.com](mailto:barathi@valencyinternational.com)  Website: [www.valencyinternational.com](http://www.valencyinternational.com/)  Visit us at |