Dear Barathi

Many thanks for the nomination and support

While we await shipment tonnage and container details our team is standby and in follow up with concerned at the site

Regards

Manoj

Get [Outlook for Android](https://aka.ms/ghei36)

**From:** Barathi <barathi@valencyinternational.com>  
**Sent:** Wednesday, 4 November 2020, 12:07  
**To:** Manoj Kewalramani  
**Cc:** Vishnu; AGRIMIN INDO; Siddharth Amin; Priyanka; Aarti Poddar; Sandar  
**Subject:** RE: Bagging - Stuffing Inspection nomination - Portklang (New Nomination) - RS Warehouse

Dear Mr. Manoj,

Refer to the whatsapp group discussion, Pls find our formal nominations:

Product: Granular urea

Location:

RS- Yal warehouse

Contact Details: Mr. Ganesh

Booking Number:

TBA

POL: Port Klang, Malaysia

POD: Yangon, Myanmar

Marking & Quantity:

Green Gold Flower

**Basic requirement for POL Inspection as follows:**

**Container:**

Checking the cleanliness of containers & its sound condition before stuffing.

Share with us the stages of picture starting from empty containers till the container sealed.

Rejection of containers that are damaged and not seaworthy.

Verification of quantity against weigh bridge slips .

Actual counting of Bags before sealing the containers.

Rejection of cargo if it deviates from the specification.

Reading of Container wise Gross Weight & Net weight.

Inspection seal is mandatory and picture to be taken to show container number & Inspection seal number & Shipping line seal number.

**Bagging:**

Ensure no **visible dirt, severely discoloured urea and lumps** are to remove.

Ensure cargo packed in bags is free flowing & cargo is as pure as possible but to maintain same packing rate as trial

Check weighing machine calibration before allowing for bagging.Net weight should be **50kgs (no minus tolerance)**

Verification of Bag marking and Bag Drop tests to ensure they are sound.

Rejection of Torn or Partial stitching bags. Bags should be double stitched.

1% of empty extra bags are required. Once stuffing complete, pls advise container number where  empty extra bags kept along with total number of empty extra bags in each container

Foreign particles limited to 1% max.

**Quality:**

The below analysis to be performed on the one composite sample taken during stuffing.

**Specifications:**

 Analysis on one composite sample drawn and the details as following:

Granular UREA

Moisture                                                       :             1.0% maximum

Nitrogen                                                       :             46% minimum

Biuret                                                             :             1.0% maximum

Physical condition                                       :             Granular, free flowing non-caking, White in colour.

PARTICLE SIZE                                               :               NOT LESS THAN 90PCT  OF THE MATERIAL SHALL PASS THROUGH A SIEVE OF APERTURE SIZE OF 4.00MM AND NOT MORE THAN 5 PERCENT OF THE MATERIAL SHALL PASSES THROUGH A SIEVE OF APERTURE SIZE OF 2MM.

...............................................................................................................................................................................................................................................................................................

**Note :**

1. Pls stop bagging or loading of cargo immediately and contact us in the event that there is deviation from any of the above requirements.
2. Inspection status to be update to us on daily basis and testing report to receive prior to the container loading into the vessel.
3. Issuance of final certificates: Certificate of Quality, Quantity and Analysis in 1 original and 2 copies.

Regards

Barathi

This email and any files transmitted with it are confidential and intended solely for the use of the individual or entity to whom they are addressed. Opinions, conclusions and other information expressed in this message are not given or endorsed by this company unless otherwise indicated by an authorized representative independent of this message. If you have received this email in error please notify us immediately. This message contains confidential information and is intended only for the individual named. This email must not be disseminated, distributed or copied