Pls create job number and let me know

Get [Outlook for Android](https://aka.ms/ghei36)

**From:** Barathi <barathi@valencyinternational.com>  
**Sent:** Tuesday, 18 August 2020, 17:56  
**To:** Manoj Kewalramani  
**Cc:** 'Vishnu, VITPL'; AGRIMIN INDO; Siddharth Amin; 'Priyanka'; 'Barathi'  
**Subject:** Stuffing Inspection nomination - Portklang

Dear Mr. Manoj,

Pls note job scope for inspection.

Product: Granular urea

Contact Details: Mr. Ganesh – Tel: +60 12-711 3530

Location:

Berjaya Baja Servis Sdn Bhd

Located at PT4231 (Lot 26725),

Lingkaran Sultan Hishamuddin,

Kawasan Perusahaan Selat Klang Utara,

42000 Pelabuhan Klang (nearby Hainan Village),

Selangor Darul Ehsan, Malaysia.

POL: Portklang, Malaysia

POD: Yangon, Myanmar

Marking & Qunatity:

Green Gold Flower Bag – 12 FCL

252 MTS

**Basic requirement for POL Inspection as follows:**

Checking the cleanliness of containers & its sound condition before stuffing.

Share with us the stages of picture starting from empty containers till the container sealed.

Rejection of containers that are damaged and not seaworthy.

Verification of Bag marking and Bag Drop tests to ensure they are sound.

Verification of quantity against weigh bridge slips .

Actual counting of Bags before sealing the containers.

Rejection of Torn or Partial stitching bags.

Rejection of cargo if it deviates from the specification.

Reading of Container wise Gross Weight & Net weight.

Inspection status has be update to us on daily basis and testing report to receive prior to the container loading into the vessel.

Plus tolerance is not acceptable. Ensure cargo loaded in minus tolerance (or unless requested by us).

Inspection seal is mandatory and picture to be taken to show container number & Inspection seal number & Shipping line seal number.

1% of empty extra bags are required. Once stuffing complete, pls advise container number where  empty extra bags kept along with total number of empty extra bags in each container

Bagging: Ensure cargo is clean, no visible dirt, Ensure no lumps in bags, net weight should be **50kgs (no tolerance)**

**Quality:**

The below analysis to be performed on the one composite sample taken during stuffing.

**Specifications:**

 Analysis on one composite sample drawn and the details as following:

Granular UREA

Moisture                                                       :             1.0% maximum

Nitrogen                                                       :             46% minimum

Biuret                                                             :             1.0% maximum

Physical condition                                       :             Granular, free flowing non-caking, grey in colour.

Particle Size                                                   :             Not less of 90 percent of the material shall pass through a sieve of nominal aperture size 4mm and shall be retained on 1mm sieve

        and not more than 5 percent shall be below 2mm. Free of lumps and visible impurities.

...............................................................................................................................................................................................................................................................................................

**Note :**

1. Pls stop loading of cargo immediately and contact us in the event that there is deviation from any of the above requirements.
2. Kindly keep us updated of cargo readiness as well as stuffing status on regular basis.
3. Results of inspections should be given to us within 2 days of inspection max.
4. Issuance of final certificates: Certificate of Quality, Quantity and Analysis in 1 original and 2 copies.

Warm Regards,

Barathi

|  |  |
| --- | --- |
|  | **Barathi**  Valency International Pte Ltd,  10 Anson Road, 18-26, International Plaza, Singapore 079903  Direct +65 6692 9487  Mobile +65 9750 8506  Board +65 6692 9460   Fx +65 6223 4252  Email: [barathi@valencyinternational.com](mailto:barathi@valencyinternational.com)  Website: [www.valencyinternational.com](http://www.valencyinternational.com/)  Visit us at |